SURFACETEXTUREmm980925/R0T.Kohriki@KEKGEN. –0.2REMOVE ALL BURRSTPGORIGINAL SCALETOLERANCES UNLESS STATEDFINISHMATERIAL & SPEC.STOCK(UNLESS STATE)1/1TITLE TPG baseboard(covered with polyimide) for KEKQUANTITY pices

4-R 2REF

42

78.6

87.6

2560652.546.529.589.5

12.5

14.25

5131.8

84.75

10.537REFf0.22-f3.8–0.12-f2.8–0.1 f0.2