.

.25 in

Detector

.2 intyp.

2.32 " ( 6 cm )

0.55 " Round StrainReliefSupportCard

5.60 "

Assemblyboard

Area For Cooling PipeDetector

2.31 "

1.242 in

1.802 inAlignment Edge

Alignment Edge 3-M 344350 pin Connector.5 in

3.25 "

3.64 "

.225 inNote 1

3.35 in

2.80 "

5.12 "

3.12 inReference

.50 in

H8 BINARY READ-OUT DETECTOR ASSEMBLY2(6 X 6)cm DETECTOR -3CDP128 Instrumented)

7.00 "

1.52 "

3 CDP128PowerConnector