Size0.5x114x114REF. 114

114

10

14

75

78

45

3.53.5172287

141082278-R0.5

2x2-R0.54-C1

SURFACE TEXTURE mm9801012/R1T.Kohriki@KEKGEN. –0.2REMOVE ALL BURRSAlumina 99.5 Thickness=0.5ORIGINAL SCALETOLERANCES UNLESS STATEDFINISHMATERIAL & SPEC.STOCK(UNLESS STATE)1/1TITLEWafer testAlumina boardQUANTITY pices