-0.500.511.522.50100200300400

Non-irrad(65V)

1.2x1014+Warmup(80V)

DC-pad

Bias resistor

Normalized responsePosition [mm]