4/12/98

Parametric simulation of the ABCD FE with TRIM DAC´s (ABCD2T)

Definition of the peaking time ( PkTim ), DELAY and WIDTH

PkTim    =  t1 - t0

DELAY  =  t2 - t0

WIDTH  =  t3 - t2

4/12/98

4/12/98

4/12/98

4/12/98

4/12/98