centre&end-tap/dec96Scale 1/1.5KEK centre-tap moduleBeO+PG/1 cooling December 10,1996/R2KEKT.Kohriki

Horizontal faceFan-inFan-inConnectorKapton hybrid with cable(Hor’l face)PG1300 baseboardwith polyimid insulatorKapton hybrid with cable(Stereo face)BeO facing

Hor’l silicon,0.3

4.5centre&end-tap/dec96Cable part

BeO bridge,0.38/1.0Kapton hybrid,0.4BeO facing,0.25Stereo silicon,0.3Thermal adhesive,0.1

130.4

63.6

85Stereo face

APG1300 baseboard with polyimid insulator,0.5 A

PG1300 baseboard with polyimid insulator,0.5

Quartz Fan-in,0.3

Section A-A Scalex2.5x5

BBSection B-B Scalex2.5x5

BeO bridge,0.38/1.0

Notes: 1.Detector =0.3 x 63.6 x 64.6 2.Rotation = 40mRad. 3.Off-set = 0 mm 4.Biasing sheme-two options 1)Use PG core as a conductor 2)Separate kapton shielded cable