77 REF.

centre/supportcard961130N-side

85.1

39.4PG700 baseboard

Solder pad

Electrically working moduleMounted on support cardN-sideCentre-tapBeO+PG/1 cooling November 30,1996/R5KEKT.KohrikiDetector =63.6 x 64.6Rotation = 40mRad.Off-set = 0 mm

134.6

144.8

165

6.4

6.422.15.1134.6Cooling plate(Aluminum plate)

BeO bridge

Kapton hybrid

177.8

161.8Unit:mmScale 1/1.2

N-side

70

P-side bias

Horizontal face

Fan-in

30.6