77 REF.

end/support961130N-side

85.1PG700 baseboard

Solder pad

Electrically working modulemounted on support cardN-sideEnd-tapPG/1 cooling November 30,1996/R2KEKT.Kohriki

134.6

144.8

82.15.1134.6

N-side

Kapton hybridHorizontal face

39.4Fan-in

6.4

177.8

221.8Detector =63.6 x 64.6Rotation = 40mRad.Off-set = 0 mm

Cooling plate(Aluminum plate)

P-side bias

30.6

6.4

165

70